; Copyright (c) 2003-14 Intel Corporation
; ****************************************************************************
; ****************************************************************************
; **    Filename:  iaAHCI.INF
; **    Revision:  Version 8.9.0.1023
; **    Date:      06/04/2009
; **    Sources:   Based on BlackWingCat mod 02/21/2014 (iata89cw2k.cab)
; **                RST v12.9.0.1001\*.inf, Chipset 9.4.4.1006\All\*ahci.inf
; **                 & http://pci-ids.ucw.cz/ (2014-12-10)
; **    Modified:  12-11-2014 by TechDud  http://forum.driverpacks.net
; **    Abstract:  Windows* INF File for Intel(R) Matrix Storage Manager Driver
; ****************************************************************************
; ****************************************************************************

[version]
; CatalogFile=iaAHCI.cat
Signature="$WINDOWS NT$"
Class=hdc
ClassGuid={4D36E96A-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
DriverVer=06/04/2009,8.9.0.1023

[SourceDisksNames]
1 = %DiskName%,,,

[SourceDisksFiles]
iaStor.sys= 1

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS
CopyFullPort = 12;

[CopyFullPort]
iaStor.sys

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%INTEL%=INTEL_HDC,NTx86.5.1

[INTEL_HDC.NTx86.5.1]
; Win2k install only

[INTEL_HDC]
; Matrix:  mobile  = DEV_xxx3,DEV_xxx5,DEV_xxx9,DEV_xxxB,DEV_xxxF
;          desktop = DEV_xxx1,DEV_xxx2,DEV_xxx4,DEV_xxx6
;
; earlier Win2k-WHQL official revision used for textmode - start
%PCI\VEN_8086&DEV_2652&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_2652&CC_0106
%PCI\VEN_8086&DEV_2653&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_2653&CC_0106
%PCI\VEN_8086&DEV_2681&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_2681&CC_0106
%PCI\VEN_8086&DEV_27C1&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_27C1&CC_0106
%PCI\VEN_8086&DEV_27C5&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_27C5&CC_0106
%PCI\VEN_8086&DEV_2821&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_2821&CC_0106
;    QEMU & VirtualBox virtual SATA HWID (8086:2829)
%PCI\VEN_8086&DEV_2829&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_2829&CC_0106
; end - earlier driver for textmode
%PCI\VEN_8086&DEV_1C02&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_1C02&CC_0106
%PCI\VEN_8086&DEV_1C03&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_1C03&CC_0106
%PCI\VEN_8086&DEV_1D02&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_1D02&CC_0106
%PCI\VEN_8086&DEV_1E02&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_1E02&CC_0106
%PCI\VEN_8086&DEV_1E03&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_1E03&CC_0106
%PCI\VEN_8086&DEV_2922&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_2922&CC_0106
%PCI\VEN_8086&DEV_2929&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_2929&CC_0106
%PCI\VEN_8086&DEV_3A02&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_3A02&CC_0106
%PCI\VEN_8086&DEV_3A22&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_3A22&CC_0106
%PCI\VEN_8086&DEV_3B22&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_3B22&CC_0106
%PCI\VEN_8086&DEV_3B29&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_3B29&CC_0106
%PCI\VEN_8086&DEV_3B2F&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_3B2F&CC_0106
%PCI\VEN_8086&DEV_5029&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_5029&CC_0106
%PCI\VEN_8086&DEV_8C02&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_8C02&CC_0106
%PCI\VEN_8086&DEV_8C03&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_8C03&CC_0106
%PCI\VEN_8086&DEV_9C02&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_9C02&CC_0106
%PCI\VEN_8086&DEV_9C03&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_9C03&CC_0106
; new section - start
%PCI\VEN_8086&DEV_0816&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_0816&CC_0106
%PCI\VEN_8086&DEV_0F22&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_0F22&CC_0106
%PCI\VEN_8086&DEV_0F23&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_0F23&CC_0106
%PCI\VEN_8086&DEV_1F22&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_1F22&CC_0106
%PCI\VEN_8086&DEV_1F23&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_1F23&CC_0106
%PCI\VEN_8086&DEV_1F32&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_1F32&CC_0106
%PCI\VEN_8086&DEV_1F33&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_1F33&CC_0106
%PCI\VEN_8086&DEV_2323&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_2323&CC_0106
%PCI\VEN_8086&DEV_23A3&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_23A3&CC_0106
%PCI\VEN_8086&DEV_24D1&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_24D1&CC_0106
%PCI\VEN_8086&DEV_2651&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_2651&CC_0106
%PCI\VEN_8086&DEV_2824&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_2824&CC_0106
%PCI\VEN_8086&DEV_2923&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_2923&CC_0106
%PCI\VEN_8086&DEV_3A03&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_3A03&CC_0106
%PCI\VEN_8086&DEV_3A23&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_3A23&CC_0106
%PCI\VEN_8086&DEV_3B23&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_3B23&CC_0106
%PCI\VEN_8086&DEV_880B&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_880B&CC_0106
%PCI\VEN_8086&DEV_8C82&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_8C82&CC_0106
%PCI\VEN_8086&DEV_8C83&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_8C83&CC_0106
%PCI\VEN_8086&DEV_8D02&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_8D02&CC_0106
%PCI\VEN_8086&DEV_8D62&CC_0106.DeviceDesc% = iaStor_Inst, PCI\VEN_8086&DEV_8D62&CC_0106
%PCI\VEN_8086&DEV_9C83&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_9C83&CC_0106
%PCI\VEN_8086&DEV_A103&CC_0106.DeviceDesc% = iaStor_mobl_Inst, PCI\VEN_8086&DEV_A103&CC_0106
; end - new section

;****************************************************
[iaStor_Inst]
AddReg = iaStor_Temp_parameters_AddReg
CopyFiles=CopyFullPort
FeatureScore=0x80

[iaStor_Inst.HW]
AddReg = iaStorSecurity.AddReg

[iaStor_mobl_Inst.HW]
AddReg = iaStorSecurity.AddReg

[iaStorSecurity.AddReg]
HKR,,Security,,"D:P(A;;FA;;;SY)(A;;FA;;;BA)(A;;FRFW;;;BU)"

[iaStor_mobl_Inst]
AddReg = iaStor_Temp_parameters_AddReg
CopyFiles=CopyFullPort
FeatureScore=0x80

[iaStor_Temp_parameters_AddReg]

[iaStor_Inst.Services]
AddService = iaStor, %SPSVCINST_ASSOCSERVICE%, iaStor_Service_Inst, iaStor_EventLog_Inst

[iaStor_mobl_Inst.Services]
AddService = iaStor, %SPSVCINST_ASSOCSERVICE%, iaStor_mobl_Service_Inst, iaStor_EventLog_Inst

[iaStor_Service_Inst]
DisplayName    = %*PNP0600.DeviceDesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\iaStor.sys
LoadOrderGroup = SCSI Miniport
AddReg         = iaStor_parameters_AddReg

[iaStor_mobl_Service_Inst]
DisplayName    = %*PNP0600.DeviceDesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\iaStor.sys
LoadOrderGroup = SCSI Miniport
AddReg         = iaStor_mobl_parameters_AddReg

[iaStor_parameters_AddReg]
HKR,,Tag,%REG_DWORD%,25
HKR,Parameters,queuePriorityEnable,%REG_DWORD%,0
HKR,Parameters,BusType,0x00010001,0x0000003

HKR,Parameters\Port0,%AN%,0x00010001,0
HKR,Parameters\Port0,%LPM%,0x00010001,0
HKR,Parameters\Port0,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port0,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port0,%GTF%,0x00010001,0
HKR,Parameters\Port0,%DIPM%,0x00010001,0

HKR,Parameters\Port1,%AN%,0x00010001,0
HKR,Parameters\Port1,%LPM%,0x00010001,0
HKR,Parameters\Port1,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port1,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port1,%GTF%,0x00010001,0
HKR,Parameters\Port1,%DIPM%,0x00010001,0

HKR,Parameters\Port2,%AN%,0x00010001,0
HKR,Parameters\Port2,%LPM%,0x00010001,0
HKR,Parameters\Port2,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port2,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port2,%GTF%,0x00010001,0
HKR,Parameters\Port2,%DIPM%,0x00010001,0

HKR,Parameters\Port3,%AN%,0x00010001,0
HKR,Parameters\Port3,%LPM%,0x00010001,0
HKR,Parameters\Port3,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port3,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port3,%GTF%,0x00010001,0
HKR,Parameters\Port3,%DIPM%,0x00010001,0

HKR,Parameters\Port4,%AN%,0x00010001,0
HKR,Parameters\Port4,%LPM%,0x00010001,0
HKR,Parameters\Port4,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port4,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port4,%GTF%,0x00010001,0
HKR,Parameters\Port4,%DIPM%,0x00010001,0

HKR,Parameters\Port5,%AN%,0x00010001,0
HKR,Parameters\Port5,%LPM%,0x00010001,0
HKR,Parameters\Port5,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port5,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port5,%GTF%,0x00010001,0
HKR,Parameters\Port5,%DIPM%,0x00010001,0

[iaStor_mobl_parameters_AddReg]
HKR,,Tag,%REG_DWORD%,25
HKR,Parameters,queuePriorityEnable,%REG_DWORD%,0
HKR,Parameters,BusType,0x00010001,0x0000003

HKR,Parameters\Port0,%AN%,0x00010001,0
HKR,Parameters\Port0,%LPM%,0x00010001,1
HKR,Parameters\Port0,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port0,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port0,%GTF%,0x00010001,1
HKR,Parameters\Port0,%DIPM%,0x00010001,1

HKR,Parameters\Port1,%AN%,0x00010001,0
HKR,Parameters\Port1,%LPM%,0x00010001,1
HKR,Parameters\Port1,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port1,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port1,%GTF%,0x00010001,1
HKR,Parameters\Port1,%DIPM%,0x00010001,1

HKR,Parameters\Port2,%AN%,0x00010001,0
HKR,Parameters\Port2,%LPM%,0x00010001,1
HKR,Parameters\Port2,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port2,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port2,%GTF%,0x00010001,1
HKR,Parameters\Port2,%DIPM%,0x00010001,1

HKR,Parameters\Port3,%AN%,0x00010001,0
HKR,Parameters\Port3,%LPM%,0x00010001,1
HKR,Parameters\Port3,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port3,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port3,%GTF%,0x00010001,1
HKR,Parameters\Port3,%DIPM%,0x00010001,1

HKR,Parameters\Port4,%AN%,0x00010001,0
HKR,Parameters\Port4,%LPM%,0x00010001,1
HKR,Parameters\Port4,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port4,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port4,%GTF%,0x00010001,1
HKR,Parameters\Port4,%DIPM%,0x00010001,1

HKR,Parameters\Port5,%AN%,0x00010001,0
HKR,Parameters\Port5,%LPM%,0x00010001,1
HKR,Parameters\Port5,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port5,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port5,%GTF%,0x00010001,1
HKR,Parameters\Port5,%DIPM%,0x00010001,1

[iaStor_EventLog_Inst]
AddReg = iaStor_EventLog_AddReg

[iaStor_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%SystemRoot%\System32\IoLogMsg.dll;%SystemRoot%\System32\drivers\iaStor.sys"
HKR,,TypesSupported,%REG_DWORD%,7

;********************************************************
[Strings]
;Localizable
DiskName                                    = "Intel Matrix Storage Manager Driver"
*PNP0600.DeviceDesc                         = "Intel AHCI Controller" ;                                                            ________From PCI ID Project at http://pci-ids.ucw.cz/. _________________Associated HW_________________________________________________________________________
; earlier Win2k-WHQL official revision used for textmode - start
PCI\VEN_8086&DEV_2652&CC_0106.DeviceDesc    = "Intel(R) 82801FR/FRW (ICH6R/ICH6RW) SATA AHCI Controller - 2652" ;                  82801FR/FRW (ICH6R/ICH6RW) SATA AHCI					(Dimension 8400, 915P/G Neo2)
PCI\VEN_8086&DEV_2653&CC_0106.DeviceDesc    = "Intel(R) 82801FBM (ICH6M) Mobile Family SATA AHCI Controller - 2653" ;              82801FBM (ICH6M) SATA AHCI
PCI\VEN_8086&DEV_2681&CC_0106.DeviceDesc    = "Intel(R) 631xESB/632xESB SATA AHCI Controller - 2681" ;                             631xESB/632xESB SATA AHCI						(ProLiant DL140 G3, X7DVL-E-O motherboard, X7DBN Motherboard, Intel S5000PSLSATA Server Board)
PCI\VEN_8086&DEV_27C1&CC_0106.DeviceDesc    = "Intel(R) 82801GR/GH (NM10/ICH7R/DH Family) SATA AHCI Controller - 27C1" ;           NM10/ICH7 Family SATA AHCI						(PowerEdge SC440,Pavilion A1512X,D270S/D250S Motherboard,Notebook N150P,GA-D525TUD,CC11/CL11,DeskTop Board D510MO,DeskTop Board D975XBX)
PCI\VEN_8086&DEV_27C5&CC_0106.DeviceDesc    = "Intel(R) 82801GBM/GHM (ICH7M/MDH) Mobile Family SATA AHCI Controller - 27C5" ;      82801GBM/GHM (ICH7-M Family) SATA AHCI				(Compaq nx9420 Notebook, Compaq nw8440, ThinkPad T60/R60 series)
PCI\VEN_8086&DEV_2821&CC_0106.DeviceDesc    = "Intel(R) 82801HR/HO/HH (ICH8R/DO/DH) 6 port SATA AHCI Controller - 2821" ;          82801HR/HO/HH (ICH8R/DO/DH) 6 port SATA AHCI
;    QEMU & VirtualBox virtual SATA HWID (8086:2829)
PCI\VEN_8086&DEV_2829&CC_0106.DeviceDesc    = "Intel(R) 82801HM/HEM (ICH8M/ICH8M-E) Mobile SATA AHCI Controller - 2829" ;          82801HM/HEM (ICH8M/ICH8M-E) SATA AHCI				(Aspire 5920G,Compaq 6710b,Compaq 6910p,Pavilion dv6700,Presario C700,Vaio VGN-FZ260E,VAIO VGN-NR120E,ThinkPad T61/R61,CCG-RUMBA)
; end - earlier driver for textmode
PCI\VEN_8086&DEV_1C02&CC_0106.DeviceDesc    = "Intel(R) Desktop/Workstation/Server Express Chipset SATA AHCI Controller" ;         6 Series/C200 Series Chipset Family SATA AHCI			(XPS 8300, P8 series motherboard, Server Board S1200BTS)
PCI\VEN_8086&DEV_1C03&CC_0106.DeviceDesc    = "Intel(R) 6 Series/C200 Mobile Express Chipset 6 port SATA AHCI Controller" ;        6 Series/C200 Series Chipset Family 6 port SATA AHCI			(Precision M4600, Vostro 3350, Vostro 3750, Apple MacBookPro8,2 [Core i7, 15", 2011])
PCI\VEN_8086&DEV_1D02&CC_0106.DeviceDesc    = "Intel(R) C600/X79 Series Chipset 6-Port SATA AHCI Controller - 1D02" ;              C600/X79 series chipset 6-Port SATA AHCI
PCI\VEN_8086&DEV_1E02&CC_0106.DeviceDesc    = "Intel(R) 7 Series/C216 Chipset Family 6-port SATA AHCI Controller - 1E02" ;         7 Series/C210 Series Chipset Family 6-port SATA AHCI			(P8H77-I Motherboard)
PCI\VEN_8086&DEV_1E03&CC_0106.DeviceDesc    = "Intel(R) 7 Series Chipset Mobile 6-port SATA AHCI Controller - 1E03" ;              7 Series Chipset Family 6-port SATA AHCI				(N56VZ, Zenbook Prime UX31A)
PCI\VEN_8086&DEV_2922&CC_0106.DeviceDesc    = "Intel(R) 82801IR/IO/IH (ICH9R/DO/DH) 6 port SATA AHCI Controller - 2922" ;          82801IR/IO/IH (ICH9R/DO/DH) 6 port SATA AHCI				(QEMU Virtual Machine (subsys_1af41100), Desktop Board DP35DP)
PCI\VEN_8086&DEV_2929&CC_0106.DeviceDesc    = "Intel(R) 82801IBM/IEM (ICH9M/ICH9M-E) 4 port SATA AHCI Controller - 2929" ;         82801IBM/IEM (ICH9M/ICH9M-E) 4 port SATA AHCI			(dv6-1190en, CCM-BOOGIE)
PCI\VEN_8086&DEV_3A02&CC_0106.DeviceDesc    = "Intel(R) 82801JD/DO (ICH10D/DO) SATA AHCI Controller - 3A02" ;                      82801JD/DO (ICH10 Family) SATA AHCI
PCI\VEN_8086&DEV_3A22&CC_0106.DeviceDesc    = "Intel(R) 82801JI (ICH10R) SATA AHCI Controller - 3A22" ;                            82801JI (ICH10 Family) SATA AHCI					(ProLiant G6 series, P5Q Deluxe Motherboard, GA-EP45-DS5/GA-EG45M-DS2H Motherboard)
PCI\VEN_8086&DEV_3B22&CC_0106.DeviceDesc    = "Intel(R) 5 Series/3400 Series Chipset 6 port SATA AHCI Controller - 3B22" ;         5 Series/3400 Series Chipset 6 port SATA AHCI			(OptiPlex 980, C7SIM-Q Motherboard)
PCI\VEN_8086&DEV_3B29&CC_0106.DeviceDesc    = "Intel(R) 5 Series/3400 Series Mobile 4 port SATA AHCI Controller - 3B29" ;          5 Series/3400 Series Chipset 4 port SATA AHCI			(Aspire 7740G)
PCI\VEN_8086&DEV_3B2F&CC_0106.DeviceDesc    = "Intel(R) 5 Series/3400 Series Chipset 6 port SATA AHCI Controller - 3B2F" ;         5 Series/3400 Series Chipset 6 port SATA AHCI			(Latitude E6510, PC1-GROOVE)
PCI\VEN_8086&DEV_5029&CC_0106.DeviceDesc    = "Intel(R) EP 80579 SATA AHCI Controller - 5029" ;                                    EP80579 SATA AHCI
PCI\VEN_8086&DEV_8C02&CC_0106.DeviceDesc    = "Intel(R) 8 Series/C220 Chipset Family 6-port SATA AHCI Controller - 8C02" ;         8 Series/C220 Series Chipset Family 6-port SATA AHCI
PCI\VEN_8086&DEV_8C03&CC_0106.DeviceDesc    = "Intel(R) 8 Series/C220 Chipset Mobile 6-port SATA AHCI Controller - 8C03" ;         8 Series/C220 Series Chipset Family 6-port SATA AHCI			(ThinkPad T440p)
PCI\VEN_8086&DEV_9C02&CC_0106.DeviceDesc    = "Intel(R) 8 Series/C220 Chipset Family SATA AHCI Controller - 9C02" ;                Lynx Point-LP SATA AHCI
PCI\VEN_8086&DEV_9C03&CC_0106.DeviceDesc    = "Intel(R) 8 Series Chipset Mobile SATA AHCI Controller - 9C03" ;                     Lynx Point-LP SATA AHCI
; new section - start
PCI\VEN_8086&DEV_0816&CC_0106.DeviceDesc    = "Intel(R) SM35 Express Chipset SATA AHCI Controller - 0816"
PCI\VEN_8086&DEV_0F22&CC_0106.DeviceDesc    = "Intel(R) Pentium(R)/Celeron(R) processor N/J-series AHCI Controller - 0F22";        ValleyView 6-Port SATA AHCI
PCI\VEN_8086&DEV_0F23&CC_0106.DeviceDesc    = "Intel(R) Pentium(R)/Celeron(R) processor N/J-series Mobile AHCI Controller - 0F23"; ValleyView 6-Port SATA AHCI
PCI\VEN_8086&DEV_1F22&CC_0106.DeviceDesc    = "Intel(R) C600+/C220+ Series SATA AHCI Controller - 1F22" ;                          Atom processor C2000 AHCI SATA2
PCI\VEN_8086&DEV_1F23&CC_0106.DeviceDesc    = "Intel(R) Atom(TM) processor C2000 product Mobile AHCI SATA 2 Controller - 1F23" ;   Atom processor C2000 AHCI SATA2
PCI\VEN_8086&DEV_1F32&CC_0106.DeviceDesc    = "Intel(R) Atom(TM) processor C2000 product family AHCI SATA 3 Controller - 1F32" ;   Atom processor C2000 AHCI SATA3
PCI\VEN_8086&DEV_1F33&CC_0106.DeviceDesc    = "Intel(R) Atom(TM) processor C2000 product Mobile AHCI SATA 3 Controller - 1F33" ;   Atom processor C2000 AHCI SATA3
PCI\VEN_8086&DEV_2323&CC_0106.DeviceDesc    = "Intel(R) DH89xxCC Series Mobile 4 port SATA AHCI Controller - 2323" ;               DH89xxCC 4 Port SATA AHCI
PCI\VEN_8086&DEV_23A3&CC_0106.DeviceDesc    = "Intel(R) Coleto Creek Mobile 4-Port SATA AHCI Controller - 23A3" ;                  Coleto Creek 4-Port SATA AHCI
PCI\VEN_8086&DEV_24D1&CC_0106.DeviceDesc    = "Intel(R) 82801EB SATA AHCI Controller - 24D1"
PCI\VEN_8086&DEV_2651&CC_0106.DeviceDesc    = "Intel(R) 82801FB (ICH6) SATA AHCI Controller - 2651"
PCI\VEN_8086&DEV_2824&CC_0106.DeviceDesc    = "Intel(R) 82801HB (ICH8) 4 port SATA AHCI Controller - 2824" ;                       82801HB (ICH8) 4 port SATA AHCI					(P5B)
PCI\VEN_8086&DEV_2923&CC_0106.DeviceDesc    = "Intel(R) 82801IB (ICH9) Mobile 4 Port SATA AHCI Controller - 2923" ;                82801IB (ICH9) 4 port SATA AHCI
PCI\VEN_8086&DEV_3A03&CC_0106.DeviceDesc    = "Intel(R) ICH10 Mobile 4 port SATA AHCI Controller - 3A03"
PCI\VEN_8086&DEV_3A23&CC_0106.DeviceDesc    = "Intel(R) ICH10 Mobile 4 port SATA AHCI Controller - 3A23"
PCI\VEN_8086&DEV_3B23&CC_0106.DeviceDesc    = "Intel(R) 5 Series/3400 Series Mobile 4 port SATA AHCI Controller - 3B23" ;          5 Series/3400 Series Chipset 4 port SATA AHCI
PCI\VEN_8086&DEV_880B&CC_0106.DeviceDesc    = "Intel(R) Platform Controller Hub EG20T Mobile SATA AHCI Controller - 880B" ;        Platform Controller Hub EG20T SATA AHCI
PCI\VEN_8086&DEV_8C82&CC_0106.DeviceDesc    = "Intel(R) 9 Series SATA AHCI Controller - 8C82"
PCI\VEN_8086&DEV_8C83&CC_0106.DeviceDesc    = "Intel(R) 9 Series Mobile SATA AHCI Controller - 8C83"
PCI\VEN_8086&DEV_8D02&CC_0106.DeviceDesc    = "Intel(R) C610/X99 Series chipset 6-Port SATA AHCI Controller - 8D02" ;              Wellsburg 6-Port SATA AHCI
PCI\VEN_8086&DEV_8D62&CC_0106.DeviceDesc    = "Intel(R) C610/X99 Series chipset sSATA AHCI Controller - 8D62" ;                    Wellsburg sSATA AHCI
PCI\VEN_8086&DEV_9C83&CC_0106.DeviceDesc    = "Intel(R) Wildcat Point-LP Mobile SATA AHCI Controller - 9C83" ;                     Wildcat Point-LP SATA AHCI
PCI\VEN_8086&DEV_A103&CC_0106.DeviceDesc    = "Intel(R) Sunrise Point-H SATA AHCI Controller - A103"
; end - new section


INTEL="Intel"
AN="AN"
LPM="LPM"
LPMSTATE="LPMSTATE"
LPMDSTATE="LPMDSTATE"
GTF="GTF"
DIPM="DIPM"

;*******************************************
;Non-Localizable
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
