; Copyright (c) 2003-12 Intel Corporation
; ****************************************************************************
; ****************************************************************************
; **    Filename:  iaAHCI.INF
; **    Revision:  Version 11.2.0.1006
; **    Date:      05/30/2012
; **    Abstract:  Windows* INF File for Intel(R) Rapid Storage Technology Driver
; ****************************************************************************
; ****************************************************************************

[version]
; CatalogFile=iaAHCI.cat
Signature="$WINDOWS NT$"
Class=hdc
ClassGUID={4D36E96A-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
DriverVer=05/30/2012,11.2.0.1006

[SourceDisksNames]
1 = %DiskName%,,,

[SourceDisksFiles]
iaStor9.sys= 1

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS
CopyFullPort = 12;

[CopyFullPort]
iaStor9.sys

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%INTEL%=INTEL_HDC,NTx86.5.1,NTx86.5.2

[INTEL_HDC]

[INTEL_HDC.NTx86.5.1]
%PCI\VEN_8086&DEV_2681&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2681&CC_0106
%PCI\VEN_8086&DEV_2821&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2821&CC_0106
%PCI\VEN_8086&DEV_2824&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2824&CC_0106
;    QEMU & VirtualBox virtual SATA HWID (8086:2829)
%PCI\VEN_8086&DEV_2829&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2829&CC_0106
%PCI\VEN_8086&DEV_2922&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2922&CC_0106
%PCI\VEN_8086&DEV_2923&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2923&CC_0106
%PCI\VEN_8086&DEV_3A03&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3A03&CC_0106
%PCI\VEN_8086&DEV_3A23&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3A23&CC_0106
%PCI\VEN_8086&DEV_3B23&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3B23&CC_0106
; added (Jan 15,2014) for testing, thanks to Fernando
%PCI\VEN_8086&DEV_0816&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_0816&CC_0106
%PCI\VEN_8086&DEV_1F22&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1F22&CC_0106 ; avotachi (below)
%PCI\VEN_8086&DEV_2323&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2323&CC_0106
%PCI\VEN_8086&DEV_8C02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8C02&CC_0106
%PCI\VEN_8086&DEV_8C03&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8C03&CC_0106
%PCI\VEN_8086&DEV_8D02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8D02&CC_0106
%PCI\VEN_8086&DEV_9C02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_9C02&CC_0106
%PCI\VEN_8086&DEV_9C03&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_9C03&CC_0106
; added (Mar 29,2014) for testing
%PCI\VEN_8086&DEV_8C82&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8C82&CC_0106
%PCI\VEN_8086&DEV_8C83&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8C83&CC_0106
; added (Nov 19,2014) for testing Based on Vista+ *AHCI.Inf files (intel chipset v9.4.4.1006)
;   avotahci.inf
%PCI\VEN_8086&DEV_1F23&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1F23&CC_0106
%PCI\VEN_8086&DEV_1F32&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1F32&CC_0106
%PCI\VEN_8086&DEV_1F33&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1F33&CC_0106
;   Tcrkahci.inf, VLV2AHCI.inf, Wellahci.inf
%PCI\VEN_8086&DEV_880B&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_880B&CC_0106
%PCI\VEN_8086&DEV_0F23&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_0F23&CC_0106
%PCI\VEN_8086&DEV_8D62&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8D62&CC_0106
;   PCI ID Project pci.ids (2014.12.10) from http://pci-ids.ucw.cz/
%PCI\VEN_8086&DEV_0F22&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_0F22&CC_0106
%PCI\VEN_8086&DEV_23A3&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_23A3&CC_0106
%PCI\VEN_8086&DEV_9C83&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_9C83&CC_0106
%PCI\VEN_8086&DEV_A103&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_A103&CC_0106
;   From iaAHCI.inf to ensure BartPE/UBCD4Win multiple concurrant driver revision support
%PCI\VEN_8086&DEV_27C1&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_27C1&CC_0106
%PCI\VEN_8086&DEV_27C5&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_27C5&CC_0106
%PCI\VEN_8086&DEV_2929&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2929&CC_0106
%PCI\VEN_8086&DEV_3A02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3A02&CC_0106
%PCI\VEN_8086&DEV_3A22&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3A22&CC_0106
%PCI\VEN_8086&DEV_3B29&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3B29&CC_0106
%PCI\VEN_8086&DEV_3B2F&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3B2F&CC_0106
%PCI\VEN_8086&DEV_3B22&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3B22&CC_0106
%PCI\VEN_8086&DEV_1C02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1C02&CC_0106
%PCI\VEN_8086&DEV_1C03&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1C03&CC_0106
%PCI\VEN_8086&DEV_1E02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1E02&CC_0106
%PCI\VEN_8086&DEV_1E03&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1E03&CC_0106


[INTEL_HDC.NTx86.5.2]
%PCI\VEN_8086&DEV_2681&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2681&CC_0106
%PCI\VEN_8086&DEV_2821&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2821&CC_0106
%PCI\VEN_8086&DEV_2824&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2824&CC_0106
;    QEMU & VirtualBox virtual SATA HWID (8086:2829)
%PCI\VEN_8086&DEV_2829&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2829&CC_0106
%PCI\VEN_8086&DEV_2922&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2922&CC_0106
%PCI\VEN_8086&DEV_2923&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2923&CC_0106
%PCI\VEN_8086&DEV_3A03&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3A03&CC_0106
%PCI\VEN_8086&DEV_3A23&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3A23&CC_0106
%PCI\VEN_8086&DEV_3B23&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3B23&CC_0106
; added (Jan 15,2014) for testing, thanks to Fernando
%PCI\VEN_8086&DEV_0816&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_0816&CC_0106
;%PCI\VEN_8086&DEV_1F22&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1F22&CC_0106 ; avotachi (below)
%PCI\VEN_8086&DEV_2323&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2323&CC_0106
;%PCI\VEN_8086&DEV_8C02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8C02&CC_0106
%PCI\VEN_8086&DEV_8C03&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8C03&CC_0106
;%PCI\VEN_8086&DEV_8D02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8D02&CC_0106
%PCI\VEN_8086&DEV_9C02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_9C02&CC_0106
%PCI\VEN_8086&DEV_9C03&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_9C03&CC_0106
; added (Mar 29,2014) for testing
%PCI\VEN_8086&DEV_8C82&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8C82&CC_0106
%PCI\VEN_8086&DEV_8C83&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8C83&CC_0106
; added (Nov 19,2014) for testing Based on Vista+ *AHCI.Inf files (intel chipset v9.4.4.1006)
;   avotahci.inf
%PCI\VEN_8086&DEV_1F23&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1F23&CC_0106
;%PCI\VEN_8086&DEV_1F32&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1F32&CC_0106
%PCI\VEN_8086&DEV_1F33&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1F33&CC_0106
;   Tcrkahci.inf, VLV2AHCI.inf, Wellahci.inf
;%PCI\VEN_8086&DEV_880B&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_880B&CC_0106
%PCI\VEN_8086&DEV_0F23&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_0F23&CC_0106
;%PCI\VEN_8086&DEV_8D62&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_8D62&CC_0106
;   PCI ID Project pci.ids (2014.12.10) from http://pci-ids.ucw.cz/
%PCI\VEN_8086&DEV_0F22&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_0F22&CC_0106
%PCI\VEN_8086&DEV_23A3&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_23A3&CC_0106
%PCI\VEN_8086&DEV_9C83&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_9C83&CC_0106
%PCI\VEN_8086&DEV_A103&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_A103&CC_0106
;   From iaAHCI.inf to ensure BartPE/UBCD4Win multiple concurrant driver revision support
%PCI\VEN_8086&DEV_27C1&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_27C1&CC_0106
%PCI\VEN_8086&DEV_27C5&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_27C5&CC_0106
%PCI\VEN_8086&DEV_2929&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_2929&CC_0106
%PCI\VEN_8086&DEV_3A02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3A02&CC_0106
%PCI\VEN_8086&DEV_3A22&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3A22&CC_0106
%PCI\VEN_8086&DEV_3B29&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3B29&CC_0106
%PCI\VEN_8086&DEV_3B2F&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3B2F&CC_0106
%PCI\VEN_8086&DEV_3B22&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_3B22&CC_0106
%PCI\VEN_8086&DEV_1C02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1C02&CC_0106
%PCI\VEN_8086&DEV_1C03&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1C03&CC_0106
%PCI\VEN_8086&DEV_1E02&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1E02&CC_0106
%PCI\VEN_8086&DEV_1E03&CC_0106.DeviceDesc% = iaStor_Install, PCI\VEN_8086&DEV_1E03&CC_0106


;****************************************************
[iaStor_Install]
AddReg = iaStor_Temp_parameters_AddReg
CopyFiles=CopyFullPort
FeatureScore=0x80

[iaStor_Install.HW]
AddReg = iaStorSecurity.AddReg

[iaStorSecurity.AddReg]
HKR,,Security,,"D:P(A;;FA;;;SY)(A;;FA;;;BA)(A;;;;;BU)"

[iaStor_Temp_parameters_AddReg]

[iaStor_Install.Services]
AddService = iaStor9, %SPSVCINST_ASSOCSERVICE%, iaStor_Service_Inst, iaStor_EventLog_Inst

[iaStor_Service_Inst]
DisplayName    = %*PNP0600.DeviceDesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\iaStor9.sys
LoadOrderGroup = SCSI Miniport
AddReg         = iaStor_parameters_AddReg

[iaStor_parameters_AddReg]
HKR,,Tag,%REG_DWORD%,25
HKR,Parameters,BusType,0x00010001,0x0000003

[iaStor_EventLog_Inst]
AddReg = iaStor_EventLog_AddReg

[iaStor_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%SystemRoot%\System32\IoLogMsg.dll;%SystemRoot%\System32\drivers\iaStor9.sys"
HKR,,TypesSupported,%REG_DWORD%,7

;********************************************************
[Strings]
;Localizable
DiskName                                    = "Intel Rapid Storage Technology Driver"
*PNP0600.DeviceDesc                         = "Intel AHCI Controller"
PCI\VEN_8086&DEV_2681&CC_0106.DeviceDesc    = "Intel(R) 631xESB/632xESB SATA AHCI Controller - 2681"
PCI\VEN_8086&DEV_2821&CC_0106.DeviceDesc    = "Intel(R) 82801HR/HO/HH (ICH8R/DO/DH) 6 port SATA AHCI Controller - 2821"
PCI\VEN_8086&DEV_2824&CC_0106.DeviceDesc    = "Intel(R) 82801HB (ICH8) 4 port SATA AHCI Controller - 2824"
PCI\VEN_8086&DEV_2829&CC_0106.DeviceDesc    = "Intel(R) 82801HM/HEM (ICH8M/ICH8M-E) Mobile SATA AHCI Controller - 2829"
PCI\VEN_8086&DEV_2922&CC_0106.DeviceDesc    = "Intel(R) 82801IR/IO/IH (ICH9R/DO/DH) 6 port SATA AHCI Controller - 2922"
PCI\VEN_8086&DEV_2923&CC_0106.DeviceDesc    = "Intel(R) 82801IB (ICH9) Mobile 4 Port SATA AHCI Controller - 2923"
PCI\VEN_8086&DEV_3A03&CC_0106.DeviceDesc    = "Intel(R) ICH10 Mobile 4 port SATA AHCI Controller - 3A03"
PCI\VEN_8086&DEV_3A23&CC_0106.DeviceDesc    = "Intel(R) ICH10 Mobile 4 port SATA AHCI Controller - 3A23"
PCI\VEN_8086&DEV_3B23&CC_0106.DeviceDesc    = "Intel(R) 5 Series/3400 Series Mobile 4 port SATA AHCI Controller - 3B23"
; added (Jan 15,2014) for testing thanks to Fernando
PCI\VEN_8086&DEV_0816&CC_0106.DeviceDesc    = "Intel(R) SM35 Express Chipset SATA AHCI Controller - 0816"
PCI\VEN_8086&DEV_1F22&CC_0106.DeviceDesc    = "Intel(R) C600+/C220+ Series SATA AHCI Controller - 1F22" ; avotachi (below)
PCI\VEN_8086&DEV_2323&CC_0106.DeviceDesc    = "Intel(R) DH89xxCC Series Mobile 4 port SATA AHCI Controller - 2323"
PCI\VEN_8086&DEV_8C02&CC_0106.DeviceDesc    = "Intel(R) 8 Series/C220 Chipset Family 6-port SATA AHCI Controller - 8C02"
PCI\VEN_8086&DEV_8C03&CC_0106.DeviceDesc    = "Intel(R) 8 Series/C220 Chipset Mobile 6-port SATA AHCI Controller - 8C03"
PCI\VEN_8086&DEV_8D02&CC_0106.DeviceDesc    = "Intel(R) C610/X99 Series chipset 6-Port SATA AHCI Controller - 8D02"
PCI\VEN_8086&DEV_9C02&CC_0106.DeviceDesc    = "Intel(R) 8 Series/C220 Chipset Family SATA AHCI Controller - 9C02"
PCI\VEN_8086&DEV_9C03&CC_0106.DeviceDesc    = "Intel(R) 8 Series Chipset Mobile SATA AHCI Controller - 9C03"
; added (Mar 29,2014) for testing
PCI\VEN_8086&DEV_8C82&CC_0106.DeviceDesc    = "Intel(R) 9 Series SATA AHCI Controller - 8C82"
PCI\VEN_8086&DEV_8C83&CC_0106.DeviceDesc    = "Intel(R) 9 Series Mobile SATA AHCI Controller - 8C83"
; added (Nov 19,2014) for testing Based on Vista AHCI .Inf files (intel chipset v9.4.4.1006)
;   avotahci.inf
PCI\VEN_8086&DEV_1F23&CC_0106.DeviceDesc    = "Intel(R) Atom(TM) processor C2000 product Mobile AHCI SATA 2 Controller - 1F23"
PCI\VEN_8086&DEV_1F32&CC_0106.DeviceDesc    = "Intel(R) Atom(TM) processor C2000 product family AHCI SATA 3 Controller - 1F32"
PCI\VEN_8086&DEV_1F33&CC_0106.DeviceDesc    = "Intel(R) Atom(TM) processor C2000 product Mobile AHCI SATA 3 Controller - 1F33"
;   Tcrkahci.inf (alt for driver in LS\), VLV2AHCI.inf, Wellahci.inf
PCI\VEN_8086&DEV_880B&CC_0106.DeviceDesc    = "Intel(R) Platform Controller Hub EG20T Mobile SATA AHCI Controller - 880B"
PCI\VEN_8086&DEV_0F23&CC_0106.DeviceDesc    = "Intel(R) Pentium(R)/Celeron(R) processor N/J-series Mobile AHCI Controller - 0F23"
PCI\VEN_8086&DEV_8D62&CC_0106.DeviceDesc    = "Intel(R) C610/X99 Series chipset sSATA AHCI Controller - 8D62"
;   PCI ID Project pci.ids (2014.12.10) from http://pci-ids.ucw.cz/
PCI\VEN_8086&DEV_0F22&CC_0106.DeviceDesc    = "Intel(R) Pentium(R)/Celeron(R) processor N/J-series AHCI Controller - 0F22"
PCI\VEN_8086&DEV_23A3&CC_0106.DeviceDesc    = "Intel(R) Coleto Creek Mobile 4-Port SATA AHCI Controller - 23A3"
PCI\VEN_8086&DEV_9C83&CC_0106.DeviceDesc    = "Intel(R) Wildcat Point-LP Mobile SATA AHCI Controller - 9C83"
PCI\VEN_8086&DEV_A103&CC_0106.DeviceDesc    = "Intel(R) Sunrise Point-H SATA AHCI Controller - A103"
;   From iaAHCI.inf to ensure BartPE/UBCD4Win multiple concurrant driver revision support
PCI\VEN_8086&DEV_27C1&CC_0106.DeviceDesc    = "Intel(R) ICH7R/DH SATA AHCI Controller"
PCI\VEN_8086&DEV_27C5&CC_0106.DeviceDesc    = "Intel(R) ICH7M/MDH SATA AHCI Controller"
PCI\VEN_8086&DEV_2929&CC_0106.DeviceDesc    = "Intel(R) ICH9M-E/M SATA AHCI Controller"
PCI\VEN_8086&DEV_3A02&CC_0106.DeviceDesc    = "Intel(R) ICH10D/DO SATA AHCI Controller"
PCI\VEN_8086&DEV_3A22&CC_0106.DeviceDesc    = "Intel(R) ICH10R SATA AHCI Controller"
PCI\VEN_8086&DEV_3B29&CC_0106.DeviceDesc    = "Intel(R) 5 Series 4 Port SATA AHCI Controller"
PCI\VEN_8086&DEV_3B2F&CC_0106.DeviceDesc    = "Intel(R) 5 Series 6 Port SATA AHCI Controller"
PCI\VEN_8086&DEV_3B22&CC_0106.DeviceDesc    = "Intel(R) 5 Series/3400 Series SATA AHCI Controller"
PCI\VEN_8086&DEV_1C02&CC_0106.DeviceDesc    = "Intel(R) Desktop/Workstation/Server Express Chipset SATA AHCI Controller"
PCI\VEN_8086&DEV_1C03&CC_0106.DeviceDesc    = "Intel(R) Mobile Express Chipset SATA AHCI Controller"
PCI\VEN_8086&DEV_1E02&CC_0106.DeviceDesc    = "Intel(R) 7 Series/C216 Chipset Family SATA AHCI Controller"
PCI\VEN_8086&DEV_1E03&CC_0106.DeviceDesc    = "Intel(R) 7 Series Chipset Family SATA AHCI Controller"

INTEL="Intel"

;*******************************************
;Non-Localizable
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
