; Disks section 
;
; The Disks section identifies the disks in the device installation kit. 
; This section has the following format:
;
; diskN = "description",tagfile,directory
;

[Disks]
DVSTXWDCX132 = "VIA StorX Driver Diskette X32 - XP", \XP\x86\VSTXWDC.TAG, \XP\x86
DVSTXWDCX164 = "VIA StorX Driver Diskette X64 - XP", \XP\x64\VSTXWDC.TAG, \XP\x64
DVSTXWDCX232 = "VIA StorX Driver Diskette X32 - SRV2003", \SRV2003\x86\VSTXWDC.TAG, \SRV2003\x86
DVSTXWDCX264 = "VIA StorX Driver Diskette X64 - SRV2003", \SRV2003\x64\VSTXWDC.TAG, \SRV2003\x64

;
; Defaults section
;
; The Defaults section lists the default driver(s) for each hardware component supported by this file. 
; Setup highlights the default selection when it presents a list of drivers to the user.
;

[Defaults]
scsi = VSTXWDC_X132

;
; HwComponent Section
;
; A HwComponent section lists the drivers available for a particular component. 
; There is a HwComponent section for each type of component supported by the file.
;

[SCSI]
VSTXWDC_X132 = "VIA StorX Controller Series (Windows XP)"
VSTXWDC_X164 = "VIA StorX Controller Series (Windows XP - X64)"
VSTXWDC_X232 = "VIA StorX Controller Series (Windows SRV2003)"
VSTXWDC_X264 = "VIA StorX Controller Series (Windows SRV2003 - X64)"

;
; Files.HwComponent.ID Section 
;
; A Files.HwComponent.ID section lists the files to be copied if the user selects a particular component option. 
; One of these sections must be present for each option listed in each HwComponent section.
;

[Files.SCSI.VSTXWDC_X132]
driver 	= DVSTXWDCX132, VSTXWDC.sys, VSTXWDC
inf    	= DVSTXWDCX132, VSTXWDC.inf
catalog = DVSTXWDCX132, VSTXWDC.cat

[Files.SCSI.VSTXWDC_X164]
driver 	= DVSTXWDCX164, VSTXWDC.sys, VSTXWDC
inf    	= DVSTXWDCX164, VSTXWDC.inf
catalog = DVSTXWDCX164, VSTXWDC.cat

[Files.SCSI.VSTXWDC_X232]
driver 	= DVSTXWDCX232, VSTXWDC.sys, VSTXWDC
inf    	= DVSTXWDCX232, VSTXWDC.inf
catalog = DVSTXWDCX232, VSTXWDC.cat

[Files.SCSI.VSTXWDC_X264]
driver 	= DVSTXWDCX264, VSTXWDC.sys, VSTXWDC
inf    	= DVSTXWDCX264, VSTXWDC.inf
catalog = DVSTXWDCX264, VSTXWDC.cat


;
; Config.DriverKey Section 
;
; A Config.DriverKey section specifies values to be set in the registry for particular component options. 
; Setup automatically creates the required values in the Services\DriverKey key. 
; Use this section to specify additional keys to be created under 
; Services\DriverKey and values under Services\DriverKey and Services\DriverKey\subkey_name.
;

[config.VSTXWDC]
value = "", EnableNcq, REG_DWORD, 1
;value = "", EnableRaid, REG_DWORD, 0
value = parameters\PnpInterface, 5, REG_DWORD, 1
value = "", DisableRaid, REG_DWORD, 0
value = "", DisableIdleDetection, REG_DWORD, 0
value = "", DisableGenRaidAwareness, REG_DWORD, 1
value = "", EnableRaidEmulation, REG_DWORD, 0
value = "", RaidEmulationType, REG_DWORD, 0
value = "", SectorNumberOfStrip, REG_DWORD, 64
value = "", CombineSequentialRwCmd, REG_DWORD, 1
value = "", DisableAtaDma, REG_DWORD, 0
value = "", DisableAtaMultiplePio, REG_DWORD, 0
value = "", DisableAtapiDma, REG_DWORD, 0
value = "", DisablePm, REG_DWORD, 13
value = "", DisableHotPlug, REG_DWORD, 0
value = "", MaxAtapiSrbTimeOutValue, REG_DWORD, 14
value = "", PreferedIpmMode, REG_DWORD, 0
value = "", PreferedIpmMethod, REG_DWORD, 0
value = "", IngoreBiosHipmSetting, REG_DWORD, 0
value = "", IngoreBiosHpIpmSetting, REG_DWORD, 0
value = "", HipmPartialPowerClock, REG_DWORD, 7
value = "", HipmSlumberPowerClock, REG_DWORD, 7
value = "", DisablePmDipm, REG_DWORD, 1
value = "", VSTXPnPPowerControl, REG_DWORD, 16
value = "", EnableG3ToG2Patch, REG_DWORD, 1


;
; HardwareIds.scsi.ID Section 
;
; A HardwareIds.scsi.ID section specifies the hardware IDs of the devices that 
; a particular mass storage driver supports. 
;

[HardwareIds.scsi.VSTXWDC_X132]
id = "PCI\VEN_1106&DEV_9000&CC_0101","VSTXWDC"
id = "PCI\VEN_1106&DEV_9001&CC_0101","VSTXWDC"

[HardwareIds.scsi.VSTXWDC_X164]
id = "PCI\VEN_1106&DEV_9000&CC_0101","VSTXWDC"
id = "PCI\VEN_1106&DEV_9001&CC_0101","VSTXWDC"

[HardwareIds.scsi.VSTXWDC_X232]
id = "PCI\VEN_1106&DEV_9000&CC_0101","VSTXWDC"
id = "PCI\VEN_1106&DEV_9001&CC_0101","VSTXWDC"

[HardwareIds.scsi.VSTXWDC_X264]
id = "PCI\VEN_1106&DEV_9000&CC_0101","VSTXWDC"
id = "PCI\VEN_1106&DEV_9001&CC_0101","VSTXWDC"

