; Copyright (c) 2003-14 Intel Corporation
; ****************************************************************************
; ****************************************************************************
; **    Filename:  iaStor.INF
; **    Revision:  Version 8.9.0.1023
; **    Date:      06/04/2009
; **    Sources:   Based on BlackWingCat mod 02/21/2014 (iata89cw2k.cab)
; **                RST v12.9.0.1001\*.inf, Chipset 9.4.4.1006\All\*ahci.inf
; **                 & http://pci-ids.ucw.cz/
; **    Modified:  11-21-2014 by TechDud  http://forum.driverpacks.net
; **    Abstract:  Windows* INF File for Intel(R) Matrix Storage Manager Driver
; ****************************************************************************
; ****************************************************************************

[version]
; CatalogFile=iaStor.cat
Signature="$WINDOWS NT$"
Class=SCSIAdapter
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
DriverVer=06/04/2009,8.9.0.1023

[SourceDisksNames]
1 = %DiskName%,,,

[SourceDisksFiles]
iaStor.sys= 1

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS
CopyFullPort = 12;

[CopyFullPort]
iaStor.sys

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%INTEL%=INTEL_HDC,ntx86

[INTEL_HDC.ntx86]
; Win2k install only

[INTEL_HDC]
; Matrix:  mobile  = DEV_xxx6,DEV_xxxA,DEV_xxxC,DEV_xxxF
;          desktop = DEV_xxx0,DEV_xxx2,DEV_xxx3,DEV_xxx5
;
; earlier Win2k-WHQL official revision used for textmode - start
%PCI\VEN_8086&DEV_24DF&CC_0104.DeviceDesc% = iaStor_Inst_RAID, PCI\VEN_8086&DEV_24DF&CC_0104
%PCI\VEN_8086&DEV_25B0&CC_0104.DeviceDesc% = iaStor_Inst_RAID, PCI\VEN_8086&DEV_25B0&CC_0104
%PCI\VEN_8086&DEV_2652&CC_0104.DeviceDesc% = iaStor_Inst_RAID, PCI\VEN_8086&DEV_2652&CC_0104
%PCI\VEN_8086&DEV_2682&CC_0104.DeviceDesc% = iaStor_Inst_RAID, PCI\VEN_8086&DEV_2682&CC_0104
%PCI\VEN_8086&DEV_27C3&CC_0104.DeviceDesc% = iaStor_Inst_RAID, PCI\VEN_8086&DEV_27C3&CC_0104
%PCI\VEN_8086&DEV_27C6&CC_0104.DeviceDesc% = iaStor_mobl_Inst_RAID, PCI\VEN_8086&DEV_27C6&CC_0104
%PCI\VEN_8086&DEV_2822&CC_0104.DeviceDesc% = iaStor_Inst_RAID, PCI\VEN_8086&DEV_2822&CC_0104
%PCI\VEN_8086&DEV_282A&CC_0104.DeviceDesc% = iaStor_mobl_Inst_RAID, PCI\VEN_8086&DEV_282A&CC_0104
; end - earlier driver for textmode
; new section - start
%PCI\VEN_8086&DEV_2683&CC_0104.DeviceDesc% = iaStor_Inst_RAID, PCI\VEN_8086&DEV_2683&CC_0104
%PCI\VEN_8086&DEV_2925&CC_0104.DeviceDesc% = iaStor_Inst_RAID, PCI\VEN_8086&DEV_2925&CC_0104
%PCI\VEN_8086&DEV_292C&CC_0104.DeviceDesc% = iaStor_mobl_Inst_RAID, PCI\VEN_8086&DEV_292C&CC_0104
%PCI\VEN_8086&DEV_3A05&CC_0104.DeviceDesc% = iaStor_Inst_RAID, PCI\VEN_8086&DEV_3A05&CC_0104
%PCI\VEN_8086&DEV_3A25&CC_0104.DeviceDesc% = iaStor_Inst_RAID, PCI\VEN_8086&DEV_3A25&CC_0104
; end - new section

;****************************************************
[iaStor_Inst_RAID]
AddReg = iaStor_Temp_parameters_AddReg
CopyFiles=CopyFullPort
FeatureScore=0x80

[iaStor_mobl_Inst_RAID]
AddReg = iaStor_Temp_parameters_AddReg
CopyFiles=CopyFullPort
FeatureScore=0x80

[iaStor_Inst_RAID.HW]
AddReg = iaStorSecurity.AddReg

[iaStor_mobl_Inst_RAID.HW]
AddReg = iaStorSecurity.AddReg

[iaStorSecurity.AddReg]
HKR,,Security,,"D:P(A;;FA;;;SY)(A;;FA;;;BA)(A;;FRFW;;;BU)"

[iaStor_Temp_parameters_AddReg]

[iaStor_Inst_RAID.Services]
AddService = iaStor, %SPSVCINST_ASSOCSERVICE%, iaStor_Service_Inst, iaStor_EventLog_Inst

[iaStor_mobl_Inst_RAID.Services]
AddService = iaStor, %SPSVCINST_ASSOCSERVICE%, iaStor_mobl_Service_Inst, iaStor_EventLog_Inst

[iaStor_Service_Inst]
DisplayName    = %*PNP0600.DeviceDesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\iaStor.sys
LoadOrderGroup = SCSI Miniport
AddReg         = iaStor_parameters_AddReg

[iaStor_mobl_Service_Inst]
DisplayName    = %*PNP0600.DeviceDesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\iaStor.sys
LoadOrderGroup = SCSI Miniport
AddReg         = iaStor_mobl_parameters_AddReg

[iaStor_parameters_AddReg]
HKR,,Tag,%REG_DWORD%,25
HKR,Parameters,queuePriorityEnable,%REG_DWORD%,0
HKR,Parameters,BusType,0x00010001,0x0000008

HKR,Parameters\Port0,%AN%,0x00010001,0
HKR,Parameters\Port0,%LPM%,0x00010001,0
HKR,Parameters\Port0,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port0,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port0,%GTF%,0x00010001,0
HKR,Parameters\Port0,%DIPM%,0x00010001,0

HKR,Parameters\Port1,%AN%,0x00010001,0
HKR,Parameters\Port1,%LPM%,0x00010001,0
HKR,Parameters\Port1,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port1,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port1,%GTF%,0x00010001,0
HKR,Parameters\Port1,%DIPM%,0x00010001,0

HKR,Parameters\Port2,%AN%,0x00010001,0
HKR,Parameters\Port2,%LPM%,0x00010001,0
HKR,Parameters\Port2,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port2,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port2,%GTF%,0x00010001,0
HKR,Parameters\Port2,%DIPM%,0x00010001,0

HKR,Parameters\Port3,%AN%,0x00010001,0
HKR,Parameters\Port3,%LPM%,0x00010001,0
HKR,Parameters\Port3,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port3,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port3,%GTF%,0x00010001,0
HKR,Parameters\Port3,%DIPM%,0x00010001,0

HKR,Parameters\Port4,%AN%,0x00010001,0
HKR,Parameters\Port4,%LPM%,0x00010001,0
HKR,Parameters\Port4,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port4,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port4,%GTF%,0x00010001,0
HKR,Parameters\Port4,%DIPM%,0x00010001,0

HKR,Parameters\Port5,%AN%,0x00010001,0
HKR,Parameters\Port5,%LPM%,0x00010001,0
HKR,Parameters\Port5,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port5,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port5,%GTF%,0x00010001,0
HKR,Parameters\Port5,%DIPM%,0x00010001,0

[iaStor_mobl_parameters_AddReg]
HKR,,Tag,%REG_DWORD%,25
HKR,Parameters,queuePriorityEnable,%REG_DWORD%,0
HKR,Parameters,BusType,0x00010001,0x0000008

HKR,Parameters\Port0,%AN%,0x00010001,0
HKR,Parameters\Port0,%LPM%,0x00010001,1
HKR,Parameters\Port0,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port0,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port0,%GTF%,0x00010001,0
HKR,Parameters\Port0,%DIPM%,0x00010001,1

HKR,Parameters\Port1,%AN%,0x00010001,0
HKR,Parameters\Port1,%LPM%,0x00010001,1
HKR,Parameters\Port1,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port1,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port1,%GTF%,0x00010001,0
HKR,Parameters\Port1,%DIPM%,0x00010001,1

HKR,Parameters\Port2,%AN%,0x00010001,0
HKR,Parameters\Port2,%LPM%,0x00010001,1
HKR,Parameters\Port2,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port2,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port2,%GTF%,0x00010001,0
HKR,Parameters\Port2,%DIPM%,0x00010001,1

HKR,Parameters\Port3,%AN%,0x00010001,0
HKR,Parameters\Port3,%LPM%,0x00010001,1
HKR,Parameters\Port3,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port3,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port3,%GTF%,0x00010001,0
HKR,Parameters\Port3,%DIPM%,0x00010001,1

HKR,Parameters\Port4,%AN%,0x00010001,0
HKR,Parameters\Port4,%LPM%,0x00010001,1
HKR,Parameters\Port4,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port4,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port4,%GTF%,0x00010001,0
HKR,Parameters\Port4,%DIPM%,0x00010001,1

HKR,Parameters\Port5,%AN%,0x00010001,0
HKR,Parameters\Port5,%LPM%,0x00010001,1
HKR,Parameters\Port5,%LPMSTATE%,0x00010001,0
HKR,Parameters\Port5,%LPMDSTATE%,0x00010001,1
HKR,Parameters\Port5,%GTF%,0x00010001,0
HKR,Parameters\Port5,%DIPM%,0x00010001,1

[iaStor_EventLog_Inst]
AddReg = iaStor_EventLog_AddReg

[iaStor_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%SystemRoot%\System32\IoLogMsg.dll;%SystemRoot%\System32\drivers\iaStor.sys"
HKR,,TypesSupported,%REG_DWORD%,7

;********************************************************
; Extra Registry Entries

[Strings]
;Localizable
DiskName                                    = "Intel Matrix Storage Manager Driver"
*PNP0600.DeviceDesc                         = "Intel RAID Controller" ;                                                     ________From PCI ID Project at http://pci-ids.ucw.cz/. _________________Associated HW_________________________________________________________________________
; earlier Win2k-WHQL official revision used for textmode - start
PCI\VEN_8086&DEV_24DF&CC_0104.DeviceDesc    = "Intel(R) 82801ER SATA RAID Controller - 24DF" ;                                         
PCI\VEN_8086&DEV_25B0&CC_0104.DeviceDesc    = "Intel(R) 6300ESB SATA RAID Controller - 25B0" ;                              6300ESB SATA RAID Controller					(CR11/VR11 Single Board Computer, Telum ASLP10 Processor AMC, PSL09 PrPMC)
PCI\VEN_8086&DEV_2652&CC_0104.DeviceDesc    = "Intel(R) 82801FR SATA RAID Controller - 2652" ;                                         
PCI\VEN_8086&DEV_2682&CC_0104.DeviceDesc    = "Intel(R) 631xESB/632xESB SATA RAID Controller - 2682" ;                      631xESB/632xESB SATA RAID						(Adaptec Serial ATA HostRAID (subsys_103c31fe))
PCI\VEN_8086&DEV_27C3&CC_0104.DeviceDesc    = "Intel(R) 82801GR/GDH (ICH7R/ICH7DH) SATA RAID Controller - 27C3" ;           82801GR/GDH (ICH7R/ICH7DH) SATA RAID				(CC11/CL11, DeskTop Board D945GTP)
PCI\VEN_8086&DEV_27C6&CC_0104.DeviceDesc    = "Intel(R) 82801GHM (ICH7-M DH) Mobile SATA RAID Controller - 27C6" ;          82801GHM (ICH7-M DH) SATA RAID
PCI\VEN_8086&DEV_2822&CC_0104.DeviceDesc    = "Intel(R) ICH8R/ICH9R/ICH10R/DO/PCH SATA RAID Controller - 2822" ;            82801HEM/HBM SATA RAID						(Inspiron 530, Asus IPIBL-LB Motherboard)
PCI\VEN_8086&DEV_282A&CC_0104.DeviceDesc    = "Intel(R) 82801HEM (ICH8M-E/9M-E/PCHM) Mobile SATA RAID Controller - 282A" ;  82801HEM Mobile SATA RAID						(Latitude E6510, PC1-GROOVE)
; end - earlier driver for textmode
; new section - start
PCI\VEN_8086&DEV_2683&CC_0104.DeviceDesc    = "Intel(R) 631xESB/632xESB SATA RAID Controller - 2683" ;                      631xESB/632xESB SATA RAID
PCI\VEN_8086&DEV_2925&CC_0104.DeviceDesc    = "Intel(R) 82801IR/IO (ICH9R/DO) SATA RAID Controller - 2925" ;                82801IR/IO (ICH9R/DO) SATA RAID					(System Board D2542)
PCI\VEN_8086&DEV_292C&CC_0104.DeviceDesc    = "Intel(R) 82801IEM (ICH9M-E) Mobile SATA RAID Controller - 292C" ;            82801IEM (ICH9M-E) SATA RAID
PCI\VEN_8086&DEV_3A05&CC_0104.DeviceDesc    = "Intel(R) 82801JD/DO (ICH10 Family) SATA RAID Controller - 3A05" ;            82801JD/DO (ICH10 Family) SATA RAID
PCI\VEN_8086&DEV_3A25&CC_0104.DeviceDesc    = "Intel(R) 82801JIR (ICH10R) SATA RAID Controller - 3A25" ;                    82801JIR (ICH10R) SATA RAID						(PERC S100 Controller (PE R410, PE T410, PE R510))
; end - new section

INTEL="Intel"
AN="AN"
LPM="LPM"
LPMSTATE="LPMSTATE"
LPMDSTATE="LPMDSTATE"
GTF="GTF"
DIPM="DIPM"

;*******************************************
;Non-Localizable
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
