AEC-6280	|	<F1> or <F10>
AEC-6293	|	<F1> or <F10>
AEC-67160	|	<F1> or <F10>
AEC-67162	|	<F1> or <F10>
AEC-6880	|	<F1> or <F10>
AEC-6885	|	Ctrl + <F1> or <F10>
AEC-6891	|	<F1> or <F10>
AEC-6897	|	<F1> or <F10>


3rdp-party controller cards with ACARD chips
are likely to use different keys.
for example:  siig uses <F3> for ATP865 (AEC-6280)