
[Disks]

d1 = "ACARD Serial ATA WINNT MINIPORT DRIVERS",winnt\aec6290.sys,winnt
d2 = "ACARD Serial ATA WIN2000 MINIPORT DRIVERS",\aec6290.sys,\
d3 = "ACARD Serial ATA WINXP MINIPORT DRIVERS",\aec6290.sys,\
d4 = "ACARD Serial ATA WIN2003 MINIPORT DRIVERS",\aec6290.sys,\

[Defaults]
SCSI=AEC6290_WinXP

# <component_name> is one of computer, display, keyboard, mouse,
#   "keyboard layout", or scsi.
#
# <id> is a unique (within the component) string to be associated
#   with an option.
#
# Example:
#
#   mouse = xyzmou1
#

[SCSI]

# Example:
#
#   [mouse]
#   xyzmou1 = "Company XYZ Mouse type 1"

AEC6290_WinNT = "ACARD AEC6290 Serial ATA WINNT MINIPORT DRIVER"
AEC6290_Win2000 = "ACARD AEC6290 Serial ATA WIN2000 MINIPORT DRIVER"
AEC6290_WinXP = "ACARD AEC6290 Serial ATA WINXP MINIPORT DRIVER"
AEC6290_Win2003 = "ACARD AEC6290 Serial ATA WIN2003 MINIPORT DRIVER"

[Files.SCSI.aec6290_WinNT]

driver = d1,aec6290.sys,aec6290_WinNT
inf    = d1,aec6290.inf

[Files.SCSI.aec6290_Win2000]

driver = d2,aec6290.sys,aec6290_Win2000
inf    = d2,aec6290.inf

[Files.SCSI.aec6290_WinXP]

driver = d3,aec6290.sys,aec6290_WinXP
inf    = d3,aec6290.inf

[Files.SCSI.aec6290_Win2003]

driver = d2,aec6290.sys,aec6290_Win2003
inf    = d2,aec6290.inf

# Example:
#
#   [Files.mouse.xyzmou1]
#   port = d1,xyzmou1p.sys,xyzmou1p


[Config.aec6290_WinNT]

[Config.aec6290_Win2000]

[Config.aec6290_WinXP]

[Config.aec6290_Win2003]


#   [Config.xyzmou1p]
#   value = "",MyValue,REG_DWORD,0
#   value = NewKey,NewValue,REG_SZ,"this is a value"

#value = <key_name>,<value_name>,<value_type>,<value>...

