#
# (C) LSI Logic Corporation
# All Rights Reserved.
#
# Windows NT 4.0 Miniport Driver for LSI LOGIC CORPORATION MegaRAID IDE
#
[Disks]
d1 = "LSI MegaRAID IDE Driver Diskette",\MegaATA,\
d2 = "LSI MegaRAID IDE Driver Diskette",\MegaATA,\Windows

[Defaults]
scsi = MegaATA_NT5

[scsi]
MegaATA_NT5 ="LSI MegaRAID IDE Driver for Windows", MegaATA

# This section lists the files that should be copied if the user
# selects a particular component option.
#
# <file_type> is one of driver, port, class, dll, hal, inf, or detect.
#   See below.
# <source_disk> identifies where the file is to be copied from, and must
#   match en entry in the [Disks] section.
# <filename> is the name of the file. This will be appended to the
#   directory specified for the disk in the [Disks] section to form the
#   full path of the file on the disk.

[Files.scsi.MegaATA_NT5]
driver  = d2, MegaATA.sys, MegaATA
inf     = d2, MegaATA.inf
inf     = d2, NODEV_MA.inf
catalog = d2, MegaATA.cat

[HardwareIds.scsi.MegaATA_NT5]
id="PCI\VEN_1095&DEV_0649&SUBSYS_0649101E", "MegaATA"
id="PCI\VEN_1095&DEV_0649&SUBSYS_005D0E11", "MegaATA"
id="PCI\VEN_1095&DEV_0649&SUBSYS_007E0E11", "MegaATA"
id="PCI\VEN_1095&DEV_0649&SUBSYS_0649101E", "MegaATA"
id="PCI\VEN_1095&DEV_0649&SUBSYS_FE001179", "MegaATA"
id="PCI\VEN_1095&DEV_0680&SUBSYS_05241000", "MegaATA"
id="PCI\VEN_1095&DEV_3112&SUBSYS_05341000", "MegaATA"
id="PCI\VEN_1166&DEV_0213&SUBSYS_02131000", "MegaATA"
id="PCI\VEN_1166&DEV_0213&SUBSYS_02131014", "MegaATA"

[Config.MegaATA]
value = "", Tag, REG_DWORD, 1
